

EQUIPMENT DESCRIPTION

2 Ball Mills







Manufacturer:




           MPSI

Type:






Wet Ball Mill

Gear and Pinion Ratio:



281:20

Speed RPM:





16.66

Diameter:





13 ft

Length:





20 ft 6 in

Material of Construction:



Rubber Lined carbon steel

2 Ball Mill motors





Manufacturer:





Reliance

Type:






WPI

Horse Power:





1750.0

Service Factor:




1.0

Voltage/Phase/Frequency:



4000/3/60

RPM:






1170

Efficiency @ 100%:




95.8

2 Gear Reducers






Manufacturer:





Falk 485A1

Gear Box Ratio:




5:1

RPM:






234

2 Gear Reducer Cooling Fan 



Manufacturer:





Falk

Wheel Diameter:




24"

2 Cooling Fan motors 





Manufacturer:





Reliance

Type:






TEFC

Horse Power:





3.0

Service Factor:




1.15

Voltage/Phase/Frequency:



575/3/60

RPM:






1750

Efficiency @ 100%:




88.5

2 Gear Reducer Air Clutch




Manufacturer:





Eaton Airflex

Type:






4VC120

2 Oil Coolers






Manufacturer:





Young

Type:






0CS-450E

2 Oil Cooler Fans






Manufacturer:





Young

Wheel Diameter:




28"

Pressure:





10058 m3/hr

2 Oil Cooler Fan motors




Manufacturer:





Siemens - RGZSD

Type:






TEFC

Horse Power:





3.0

Service Factor:




1.15

Voltage/Phase/Frequency:



575/3/60

RPM:






1200

Efficiency @ 100%:




N/A

2 Oil Reservoir Tank





Manufacturer:





Young

Capacity:





416 litre

4 Circ. Oil Pump






Manufacturer:





Viking - series 75


Speed RPM:





1200

Capacity:





1600 l/hr

4 Circ. Oil Pump Motors




Manufacturer:





Reliance

Type:






TEFC

Horse Power:





2.0

Service Factor:




1.15

Voltage/Phase/Frequency:



575/3/60

RPM:






1200

Efficiency @ 100%:




87.5

2 Oil Reservoir Heaters





Manufacturer:





Chromalox

kW Rating:





3.0

Voltage/Phase/Frequency:



575/3/60

2 Air Receivers






Manufacturer:





Teledyne

Height:





48"

Diameter:





20"

Design Pressure:




860 kPa

2 Bearing Lift Pump





Manufacturer:





Dynex/Rivett

Model #:





PF 1002-2978

Speed RPM:





1200

Capacity:





300.0 l/hr

2 Bearing Lift Pump Motors




Manufacturer:





Reliance

Type:






TEFC

Horse Power:





3.0

Service Factor:




1.15

Voltage/Phase/Frequency:



575/3/60

RPM:






1200

Efficiency @ 100%:




89.5


